#N canvas 4 80 664 396 10;
#X obj -104 176 cnv 15 100 60 empty empty empty 20 12 0 14 -4034 -66577
0;
#X obj -85 190 unpackOSC;
#X floatatom 16 207 10 0 0 1 - - -;
#X obj -85 257 pipelist;
#X text -126 337 see:;
#X text 21 337 for a way to send OSC over TCP or serial connections.
;
#X obj -91 338 unpackOSCstream;
#X obj -92 214 print unpacked;
#X text -29 253 If the OSC packet has a timetag \, [pipelist] will
delay it until the time occurs;
#N canvas 521 651 494 344 META 0;
#X text 12 155 HELP_PATCH_AUTHORS "pd meta" information added by Jonathan
Wilkes for Pd version 0.42.;
#X text 12 25 LICENSE GPL v2 or later;
#X text 12 5 KEYWORDS control list_op;
#X text 12 45 DESCRIPTION parses lists of floats (only integers on
[0..255]) assuming they represent OSC packets.;
#X text 12 75 INLET_0 list of floats on [0..255];
#X text 12 95 OUTLET_0 OSC message;
#X text 13 115 OUTLET_1 milliseconds until timetag time;
#X text 12 135 AUTHOR Martin Peach;
#X restore 449 362 pd META;
#X obj -85 73 packOSC;
#X obj -62 113 print bytes;
#X msg -113 28 /some/path 1 2 3;
#X msg -134 7 [ \, /another/one/ 4 \, ];
#X obj -85 284 print delayed;
#X msg -92 49 timetagoffset 1.1e+06;
#X obj -46 93 print bundle_depth;
#X text 354 317 2012/02/14 Martin Peach;
#X text 107 15 [unpackOSC] processes lists of floats (only integers
on [0..255]) as though they were OSC packets.;
#X text -76 134 <- usually the bytes pass over the network with [udpsend]/[udpreceive]
\, or serial port using [comport] with [slipenc] and [slipdec];
#X text 48 49 timetag offset is in microseconds relative to sender's
clock;
#X text 83 201 second outlet is timetag offset in millieconds relative
to receiver's clock;
#X connect 1 0 3 0;
#X connect 1 0 7 0;
#X connect 1 1 2 0;
#X connect 1 1 3 1;
#X connect 3 0 14 0;
#X connect 10 0 11 0;
#X connect 10 0 1 0;
#X connect 10 1 16 0;
#X connect 12 0 10 0;
#X connect 13 0 10 0;
#X connect 15 0 10 0;
