#N canvas 780 397 1010 504 12;
#X floatatom 414 304 3 0 0 0 - - -, f 3;
#X floatatom 441 304 3 0 0 0 - - -, f 3;
#X floatatom 468 304 3 0 0 0 - - -, f 3;
#X floatatom 495 304 3 0 0 0 - - -, f 3;
#X floatatom 522 305 5 0 0 0 - - -, f 5;
#X obj 414 278 unpack 0 0 0 0 0;
#X msg 191 90 status;
#X floatatom 293 225 9 0 0 0 - - -, f 9;
#X obj 474 251 tgl 15 0 empty empty empty 17 7 0 10 -4034 -1 -1 0 1
;
#X floatatom 353 251 9 0 0 0 - - -, f 9;
#X text -10 90 get status on right outlet:;
#X text 186 225 bytes received:;
#X text 201 249 total bytes received:;
#X text 371 303 from:;
#X text 293 78 Specify a multicast address (from 224.0.0.0 to 239.255.255.255)
to use multicasting;
#X text 36 38 Creation arguments: port number to listen on (required)
;
#X obj 191 294 spigot;
#X obj 230 274 tgl 15 0 empty empty enable_print: -77 8 0 10 -4034
-1 -1 0 1;
#X obj 293 192 route received total from multicast;
#X text 175 56 IP address to listen on (optional);
#X msg 202 129 port 9998;
#X text 276 127 change port to listen on;
#X text 486 360 Martin Peach 2010/10/15;
#X text -12 3 [udpreceive] receives datagrams over a udp connection
and outputs them as raw bytes.;
#N canvas 529 53 494 344 META 0;
#X text 12 155 HELP_PATCH_AUTHORS "pd meta" information added by Jonathan
Wilkes for Pd version 0.42.;
#X text 12 25 LICENSE GPL v2 or later;
#X text 12 135 AUTHOR Martin Peach;
#X text 12 5 KEYWORDS control network;
#X text 12 45 DESCRIPTION receive datagrams over a udp connection and
outputs them as raw bytes;
#X text 12 75 INLET_0 status port;
#X text 12 95 OUTLET_0 anything;
#X text 12 115 OUTLET_1 received total from multicast;
#X restore 657 396 pd META;
#X obj 73 265 realtime;
#X obj 87 221 t b b;
#X floatatom 75 293 5 0 0 0 - - -, f 5;
#X floatatom 84 395 5 0 0 0 - - -, f 5;
#X obj 85 367 t f f;
#X obj 13 369 t f f;
#X floatatom 13 394 5 0 0 0 - - -, f 5;
#X obj 12 345 min 100;
#X obj 102 344 max;
#X obj 191 319 moocow/bytes2any;
#X obj 190 159 mrpeach/udpreceive 8000;
#X obj 200 373 vsl 10 50 0 1024 0 0 empty empty empty 0 -9 0 10 -262144
-1 -1 0 1;
#X obj 215 392 realtime;
#X obj 215 368 t b b;
#X floatatom 215 415 5 0 0 0 - - -, f 5;
#X obj 200 344 route UKI_ESP_1;
#X obj 320 423 vsl 10 50 0 1024 0 0 empty empty empty 0 -9 0 10 -262144
-1 -1 0 1;
#X obj 335 442 realtime;
#X obj 335 418 t b b;
#X floatatom 335 465 5 0 0 0 - - -, f 5;
#X floatatom 155 378 5 0 0 0 - - -, f 5;
#X obj 320 394 route UKI_ESP_2;
#X obj 404 361 print received;
#X obj 620 242 mrpeach/udpsend;
#X msg 634 164 48 49 50;
#X floatatom 148 337 5 0 0 0 - - -, f 5;
#X msg 624 209 disconnect \, connect 192.168.1.255 9000;
#X connect 5 0 0 0;
#X connect 5 1 1 0;
#X connect 5 2 2 0;
#X connect 5 3 3 0;
#X connect 5 4 4 0;
#X connect 6 0 35 0;
#X connect 16 0 34 0;
#X connect 17 0 16 1;
#X connect 18 0 7 0;
#X connect 18 1 9 0;
#X connect 18 2 5 0;
#X connect 18 3 8 0;
#X connect 20 0 35 0;
#X connect 25 0 27 0;
#X connect 25 0 32 0;
#X connect 25 0 33 0;
#X connect 26 0 25 0;
#X connect 26 1 25 1;
#X connect 29 0 28 0;
#X connect 29 1 33 1;
#X connect 30 0 31 0;
#X connect 30 1 32 1;
#X connect 32 0 30 0;
#X connect 33 0 29 0;
#X connect 34 0 40 0;
#X connect 35 0 16 0;
#X connect 35 0 26 0;
#X connect 35 1 18 0;
#X connect 37 0 39 0;
#X connect 38 0 37 0;
#X connect 38 1 37 1;
#X connect 40 0 36 0;
#X connect 40 0 38 0;
#X connect 40 0 50 0;
#X connect 40 1 46 0;
#X connect 42 0 44 0;
#X connect 43 0 42 0;
#X connect 43 1 42 1;
#X connect 46 0 41 0;
#X connect 46 0 43 0;
#X connect 46 1 47 0;
#X connect 49 0 48 0;
#X connect 51 0 48 0;
