(export (version D)
  (design
    (source "/home/titi/work/projets/Fresnoy/Hadrien Tequi/HTequi/PCB/BLOBCNC_LOW/BLOBCNC_LOW.sch")
    (date "lun. 20 mai 2019 00:29:24 CEST")
    (tool "Eeschema 5.0.0+dfsg1-2")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source BLOBCNC_LOW.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U2)
      (value 74HCT125N)
      (footprint Package_DIP:DIP-14_W7.62mm_Socket_LongPads)
      (libsource (lib Lien) (part 74HCT125N) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB8813C))
    (comp (ref Q1)
      (value IRLIZ44N)
      (footprint Package_TO_SOT_THT:TO-220F-3_Vertical)
      (datasheet http://www.irf.com/product-info/datasheets/data/irliz44n.pdf)
      (libsource (lib Transistor_FET) (part IRLIZ44N) (description "30A Id, 55V Vds, Single N-Channel HEXFET Power MOSFET, 22mOhm Ron, TO-220AB"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CB8825A))
    (comp (ref U6)
      (value Teensy3.5)
      (footprint Lien:Teensy35_36_base)
      (libsource (lib teensy) (part Teensy3.5) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBEFFB4))
    (comp (ref U1)
      (value W5500)
      (footprint Lien:W5500)
      (libsource (lib Lien) (part W5500) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBF06B1))
    (comp (ref J1)
      (value LedOut)
      (footprint TerminalBlock:TerminalBlock_bornier-2_P5.08mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBF0EE1))
    (comp (ref J6)
      (value Conn_01x03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBF26E8))
    (comp (ref U7)
      (value DC-DC_MP1584EN)
      (footprint Lien:DC-DC_MP1584EN)
      (libsource (lib Lien) (part DC-DC_MP1584EN) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBF2AA4))
    (comp (ref J2)
      (value Conn_01x06)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x06) (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBF9B09))
    (comp (ref U3)
      (value 74HCT125N)
      (footprint Package_DIP:DIP-14_W7.62mm_Socket_LongPads)
      (libsource (lib Lien) (part 74HCT125N) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC00746))
    (comp (ref J3)
      (value Conn_01x06)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x06) (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC0076C))
    (comp (ref U4)
      (value 74HCT125N)
      (footprint Package_DIP:DIP-14_W7.62mm_Socket_LongPads)
      (libsource (lib Lien) (part 74HCT125N) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC028D8))
    (comp (ref J4)
      (value Conn_01x06)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x06) (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC028FE))
    (comp (ref U5)
      (value 74HCT125N)
      (footprint Package_DIP:DIP-14_W7.62mm_Socket_LongPads)
      (libsource (lib Lien) (part 74HCT125N) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC1891F))
    (comp (ref J5)
      (value Conn_01x06)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x06) (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CC18945))
    (comp (ref R1)
      (value 10k)
      (footprint Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal)
      (datasheet ~)
      (libsource (lib Device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDBBFD6))
    (comp (ref J7)
      (value Conn_01x03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDE1661))
    (comp (ref J8)
      (value Conn_01x03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDEDFE5))
    (comp (ref J9)
      (value Conn_01x03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDEDFEC))
    (comp (ref J10)
      (value Conn_01x03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDFAA57))
    (comp (ref J11)
      (value Conn_01x03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDFAA5F))
    (comp (ref J12)
      (value Conn_01x03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDFAA66))
    (comp (ref J13)
      (value Conn_01x03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CDFAA6D))
    (comp (ref J14)
      (value Conn_01x03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE075EA))
    (comp (ref J15)
      (value Conn_01x03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE075F1))
    (comp (ref J16)
      (value Conn_01x03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE075F8))
    (comp (ref J17)
      (value Conn_01x03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE07600))
    (comp (ref J18)
      (value Conn_01x03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE07607))
    (comp (ref J19)
      (value Conn_01x03)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x03) (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CE0760E))
    (comp (ref J20)
      (value +12V)
      (footprint TerminalBlock:TerminalBlock_bornier-2_P5.08mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x02) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5CBF0AED)))
  (libparts
    (libpart (lib Connector_Generic) (part Conn_01x02)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x03)
      (description "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x03))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))))
    (libpart (lib Connector_Generic) (part Conn_01x06)
      (description "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x06))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib Device) (part R)
      (description Resistor)
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Lien) (part 74HCT125N)
      (fields
        (field (name Reference) U)
        (field (name Value) 74HCT125N))
      (pins
        (pin (num 1) (name 1!OE) (type input))
        (pin (num 2) (name 1A) (type input))
        (pin (num 3) (name 1Y) (type output))
        (pin (num 4) (name 2!OE) (type input))
        (pin (num 5) (name 2A) (type input))
        (pin (num 6) (name 2Y) (type output))
        (pin (num 7) (name GND) (type power_in))
        (pin (num 8) (name 3Y) (type output))
        (pin (num 9) (name 3A) (type input))
        (pin (num 10) (name 3!OE) (type input))
        (pin (num 11) (name 4Y) (type output))
        (pin (num 12) (name 4A) (type input))
        (pin (num 13) (name 4!OE) (type input))
        (pin (num 14) (name Vcc) (type power_in))))
    (libpart (lib Lien) (part DC-DC_MP1584EN)
      (fields
        (field (name Reference) U)
        (field (name Value) DC-DC_MP1584EN))
      (pins
        (pin (num 1) (name GND_IN) (type power_in))
        (pin (num 2) (name Vcc_IN) (type power_in))
        (pin (num 3) (name GND_OUT) (type power_out))
        (pin (num 4) (name Vcc_OUT) (type power_out))))
    (libpart (lib Lien) (part W5500)
      (fields
        (field (name Reference) U)
        (field (name Value) W5500))
      (pins
        (pin (num 1) (name Gnd) (type power_in))
        (pin (num 2) (name MOSI) (type input))
        (pin (num 3) (name SCK) (type input))
        (pin (num 4) (name CS) (type input))
        (pin (num 5) (name INT) (type output))
        (pin (num 6) (name MISO) (type output))
        (pin (num 7) (name RST) (type input))
        (pin (num 8) (name 3V3) (type power_in))))
    (libpart (lib Transistor_FET) (part IRLIZ44N)
      (description "30A Id, 55V Vds, Single N-Channel HEXFET Power MOSFET, 22mOhm Ron, TO-220AB")
      (docs http://www.irf.com/product-info/datasheets/data/irliz44n.pdf)
      (footprints
        (fp TO?220F*))
      (fields
        (field (name Reference) Q)
        (field (name Value) IRLIZ44N)
        (field (name Footprint) Package_TO_SOT_THT:TO-220F-3_Vertical))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name D) (type passive))
        (pin (num 3) (name S) (type passive))))
    (libpart (lib teensy) (part Teensy3.5)
      (fields
        (field (name Reference) U)
        (field (name Value) Teensy3.5))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name 0_RX1_MOSI1_Touch) (type BiDi))
        (pin (num 3) (name 1_TX1_MISO1_Touch) (type BiDi))
        (pin (num 4) (name 2_PWM) (type BiDi))
        (pin (num 5) (name 3_PWM_CAN0TX_SCL2) (type BiDi))
        (pin (num 6) (name 4_PWM_CAN0RX_SDA2) (type BiDi))
        (pin (num 7) (name 5_PWM_tx1_miso1) (type BiDi))
        (pin (num 8) (name 6_PWM) (type BiDi))
        (pin (num 9) (name 7_RX3_miso0_scl0) (type BiDi))
        (pin (num 10) (name 8_TX3_miso0_sda0) (type BiDi))
        (pin (num 11) (name 9_PWM_RX2_CS0) (type BiDi))
        (pin (num 12) (name 10_PWM_TX2_CS0) (type BiDi))
        (pin (num 13) (name 11_MOSI0) (type BiDi))
        (pin (num 14) (name 12_MISO0) (type BiDi))
        (pin (num 15) (name 3.3V) (type power_out))
        (pin (num 16) (name 24) (type BiDi))
        (pin (num 17) (name 25) (type BiDi))
        (pin (num 18) (name 26_tx1) (type BiDi))
        (pin (num 19) (name 27_rx1) (type BiDi))
        (pin (num 20) (name 28) (type BiDi))
        (pin (num 21) (name 29_PWM_can0tx_Touch) (type BiDi))
        (pin (num 22) (name 30_PWM_can0rx_Touch) (type BiDi))
        (pin (num 23) (name 31_A12_RX4_CS1) (type BiDi))
        (pin (num 24) (name 32_A13_TX4_SCK1) (type BiDi))
        (pin (num 25) (name VBat) (type power_in))
        (pin (num 26) (name 3.3V) (type power_in))
        (pin (num 27) (name GND) (type power_in))
        (pin (num 28) (name Program) (type input))
        (pin (num 29) (name Reset) (type input))
        (pin (num 30) (name 33_A14_CAN1TX_scl0) (type BiDi))
        (pin (num 31) (name 34_A15_CAN1TX_sda0) (type BiDi))
        (pin (num 32) (name 35_A16_PWM) (type BiDi))
        (pin (num 33) (name 36_A17_PWM) (type BiDi))
        (pin (num 34) (name 37_A18_PWM_SCL1) (type BiDi))
        (pin (num 35) (name 38_A19_PWM_SDA1) (type BiDi))
        (pin (num 36) (name 39_A20) (type BiDi))
        (pin (num 37) (name A21_DAC0) (type BiDi))
        (pin (num 38) (name A22_DAC1) (type BiDi))
        (pin (num 39) (name GND) (type power_in))
        (pin (num 40) (name 13_SCK0_LED) (type BiDi))
        (pin (num 41) (name 14_A0_PWM_sck0) (type BiDi))
        (pin (num 42) (name 15_A1_CS0_Touch) (type BiDi))
        (pin (num 43) (name 16_A2_scl0_Touch) (type BiDi))
        (pin (num 44) (name 17_A3_sda0_Touch) (type BiDi))
        (pin (num 45) (name 18_A4_SDA0_Touch) (type BiDi))
        (pin (num 46) (name 19_A5_SCL0_Touch) (type BiDi))
        (pin (num 47) (name 20_A6_PWM_CS0_sck1) (type BiDi))
        (pin (num 48) (name 21_A7_PWM_CS0_sck1) (type BiDi))
        (pin (num 49) (name 22_A8_PWM_Touch) (type BiDi))
        (pin (num 50) (name 23_A9_PWM_Touch) (type BiDi))
        (pin (num 51) (name 3.3V_max250mA) (type power_out))
        (pin (num 52) (name AGND) (type power_out))
        (pin (num 53) (name Vin) (type power_in))
        (pin (num 54) (name VUSB) (type power_in))
        (pin (num 55) (name AREF) (type input))
        (pin (num 56) (name A10) (type BiDi))
        (pin (num 57) (name A11) (type BiDi))
        (pin (num 58) (name not_used) (type NotConnected))
        (pin (num 59) (name A26_D-) (type BiDi))
        (pin (num 60) (name A25_D+) (type BiDi))
        (pin (num 61) (name GND) (type power_in))
        (pin (num 62) (name GND) (type power_in))
        (pin (num 63) (name G) (type power_in))
        (pin (num 64) (name Debug_DE) (type input))
        (pin (num 65) (name Debug_DC) (type input))
        (pin (num 66) (name Debug_DD) (type input))
        (pin (num 67) (name 40) (type BiDi))
        (pin (num 68) (name 41) (type BiDi))
        (pin (num 69) (name 42) (type BiDi))
        (pin (num 70) (name 43_CS2) (type BiDi))
        (pin (num 71) (name 44_MOSI2) (type BiDi))
        (pin (num 72) (name 45_MISO2) (type BiDi))
        (pin (num 73) (name 46_SCK2) (type BiDi))
        (pin (num 74) (name GND) (type power_in))
        (pin (num 75) (name 3.3V) (type power_in))
        (pin (num 76) (name 47_RX6_SCL0) (type BiDi))
        (pin (num 77) (name 48_TX6_SDA0) (type BiDi))
        (pin (num 78) (name 49_A23) (type BiDi))
        (pin (num 79) (name 50_A24) (type BiDi))
        (pin (num 80) (name 51_MISO2) (type BiDi))
        (pin (num 81) (name 52_MOSI2) (type BiDi))
        (pin (num 82) (name 53_SCK2) (type BiDi))
        (pin (num 83) (name 54_CS2) (type BiDi))
        (pin (num 84) (name 55) (type BiDi))
        (pin (num 85) (name 56) (type BiDi))
        (pin (num 86) (name 57) (type BiDi)))))
  (libraries
    (library (logical Connector_Generic)
      (uri /usr/share/kicad/library/Connector_Generic.lib))
    (library (logical Device)
      (uri /usr/share/kicad/library/Device.lib))
    (library (logical Lien)
      (uri /home/titi/work/dev/pcb/kicad_lien/kicad_lien.lib))
    (library (logical Transistor_FET)
      (uri /usr/share/kicad/library/Transistor_FET.lib))
    (library (logical teensy)
      (uri /home/titi/work/dev/pcb/kicad_lib/teensy_library/teensy.lib)))
  (nets
    (net (code 1) (name +5V)
      (node (ref U4) (pin 14))
      (node (ref J3) (pin 4))
      (node (ref J3) (pin 6))
      (node (ref J19) (pin 2))
      (node (ref J17) (pin 2))
      (node (ref J18) (pin 2))
      (node (ref J4) (pin 6))
      (node (ref J4) (pin 4))
      (node (ref J4) (pin 2))
      (node (ref U6) (pin 53))
      (node (ref J3) (pin 2))
      (node (ref U3) (pin 14))
      (node (ref U7) (pin 4))
      (node (ref U2) (pin 14))
      (node (ref J12) (pin 2))
      (node (ref J5) (pin 6))
      (node (ref J15) (pin 2))
      (node (ref J14) (pin 2))
      (node (ref J5) (pin 4))
      (node (ref J5) (pin 2))
      (node (ref J9) (pin 2))
      (node (ref J10) (pin 2))
      (node (ref J2) (pin 2))
      (node (ref J2) (pin 4))
      (node (ref J11) (pin 2))
      (node (ref J2) (pin 6))
      (node (ref J13) (pin 2))
      (node (ref J6) (pin 2))
      (node (ref U5) (pin 14))
      (node (ref J16) (pin 2))
      (node (ref J7) (pin 2))
      (node (ref J8) (pin 2)))
    (net (code 2) (name "Net-(J1-Pad1)")
      (node (ref Q1) (pin 2))
      (node (ref J1) (pin 1)))
    (net (code 3) (name GND)
      (node (ref U1) (pin 1))
      (node (ref J6) (pin 1))
      (node (ref U7) (pin 3))
      (node (ref U7) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref U2) (pin 7))
      (node (ref U5) (pin 1))
      (node (ref U5) (pin 12))
      (node (ref U5) (pin 7))
      (node (ref U5) (pin 4))
      (node (ref U5) (pin 10))
      (node (ref U2) (pin 10))
      (node (ref U4) (pin 1))
      (node (ref U4) (pin 10))
      (node (ref U4) (pin 12))
      (node (ref U4) (pin 4))
      (node (ref U4) (pin 7))
      (node (ref U3) (pin 1))
      (node (ref U3) (pin 10))
      (node (ref U3) (pin 12))
      (node (ref U3) (pin 4))
      (node (ref U6) (pin 1))
      (node (ref Q1) (pin 3))
      (node (ref U2) (pin 4))
      (node (ref U3) (pin 7))
      (node (ref U2) (pin 12))
      (node (ref J7) (pin 1))
      (node (ref J8) (pin 1))
      (node (ref J17) (pin 1))
      (node (ref J18) (pin 1))
      (node (ref J19) (pin 1))
      (node (ref J20) (pin 1))
      (node (ref J16) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref J15) (pin 1))
      (node (ref J14) (pin 1))
      (node (ref J13) (pin 1))
      (node (ref J12) (pin 1))
      (node (ref J11) (pin 1))
      (node (ref J10) (pin 1))
      (node (ref J9) (pin 1)))
    (net (code 4) (name "Net-(U5-Pad2)")
      (node (ref U6) (pin 22))
      (node (ref U5) (pin 2)))
    (net (code 5) (name "Net-(U5-Pad5)")
      (node (ref U6) (pin 23))
      (node (ref U5) (pin 5)))
    (net (code 6) (name "Net-(U5-Pad9)")
      (node (ref U5) (pin 9))
      (node (ref U6) (pin 24)))
    (net (code 7) (name "Net-(U6-Pad20)")
      (node (ref U6) (pin 20)))
    (net (code 8) (name "Net-(U3-Pad5)")
      (node (ref U3) (pin 5))
      (node (ref U6) (pin 6)))
    (net (code 9) (name "Net-(U2-Pad5)")
      (node (ref U6) (pin 3))
      (node (ref U2) (pin 5)))
    (net (code 10) (name "Net-(U2-Pad9)")
      (node (ref U6) (pin 4))
      (node (ref U2) (pin 9)))
    (net (code 11) (name "Net-(U3-Pad2)")
      (node (ref U6) (pin 5))
      (node (ref U3) (pin 2)))
    (net (code 12) (name "Net-(U3-Pad9)")
      (node (ref U6) (pin 7))
      (node (ref U3) (pin 9)))
    (net (code 13) (name "Net-(U4-Pad2)")
      (node (ref U6) (pin 8))
      (node (ref U4) (pin 2)))
    (net (code 14) (name "Net-(J5-Pad3)")
      (node (ref J5) (pin 3))
      (node (ref U5) (pin 6)))
    (net (code 15) (name "Net-(J5-Pad5)")
      (node (ref J5) (pin 5))
      (node (ref U5) (pin 8)))
    (net (code 16) (name "Net-(J5-Pad1)")
      (node (ref J5) (pin 1))
      (node (ref U5) (pin 3)))
    (net (code 17) (name "Net-(U2-Pad2)")
      (node (ref U2) (pin 2))
      (node (ref U6) (pin 2)))
    (net (code 18) (name "Net-(U6-Pad18)")
      (node (ref U6) (pin 18)))
    (net (code 19) (name "Net-(U6-Pad17)")
      (node (ref U6) (pin 17)))
    (net (code 20) (name "Net-(Q1-Pad1)")
      (node (ref U6) (pin 21))
      (node (ref Q1) (pin 1))
      (node (ref R1) (pin 2)))
    (net (code 21) (name +12V)
      (node (ref J20) (pin 2))
      (node (ref U7) (pin 2))
      (node (ref J1) (pin 2)))
    (net (code 22) (name "Net-(U1-Pad4)")
      (node (ref U1) (pin 4))
      (node (ref U6) (pin 12)))
    (net (code 23) (name "Net-(U4-Pad5)")
      (node (ref U6) (pin 9))
      (node (ref U4) (pin 5)))
    (net (code 24) (name "Net-(U4-Pad9)")
      (node (ref U6) (pin 10))
      (node (ref U4) (pin 9)))
    (net (code 25) (name "Net-(U6-Pad11)")
      (node (ref U6) (pin 11)))
    (net (code 26) (name "Net-(U6-Pad16)")
      (node (ref U6) (pin 16)))
    (net (code 27) (name "Net-(U6-Pad55)")
      (node (ref U6) (pin 55)))
    (net (code 28) (name "Net-(J6-Pad3)")
      (node (ref J6) (pin 3))
      (node (ref U6) (pin 47)))
    (net (code 29) (name "Net-(U6-Pad37)")
      (node (ref U6) (pin 37)))
    (net (code 30) (name "Net-(U6-Pad38)")
      (node (ref U6) (pin 38)))
    (net (code 31) (name "Net-(U6-Pad39)")
      (node (ref U6) (pin 39)))
    (net (code 32) (name "Net-(U6-Pad40)")
      (node (ref U6) (pin 40)))
    (net (code 33) (name "Net-(U6-Pad48)")
      (node (ref U6) (pin 48)))
    (net (code 34) (name "Net-(U6-Pad49)")
      (node (ref U6) (pin 49)))
    (net (code 35) (name "Net-(U6-Pad50)")
      (node (ref U6) (pin 50)))
    (net (code 36) (name "Net-(U6-Pad51)")
      (node (ref U6) (pin 51)))
    (net (code 37) (name "Net-(U6-Pad52)")
      (node (ref U6) (pin 52)))
    (net (code 38) (name "Net-(U6-Pad54)")
      (node (ref U6) (pin 54)))
    (net (code 39) (name "Net-(U6-Pad56)")
      (node (ref U6) (pin 56)))
    (net (code 40) (name "Net-(U6-Pad57)")
      (node (ref U6) (pin 57)))
    (net (code 41) (name "Net-(U6-Pad59)")
      (node (ref U6) (pin 59)))
    (net (code 42) (name "Net-(U6-Pad60)")
      (node (ref U6) (pin 60)))
    (net (code 43) (name "Net-(U6-Pad61)")
      (node (ref U6) (pin 61)))
    (net (code 44) (name "Net-(U6-Pad62)")
      (node (ref U6) (pin 62)))
    (net (code 45) (name "Net-(U6-Pad63)")
      (node (ref U6) (pin 63)))
    (net (code 46) (name "Net-(U6-Pad64)")
      (node (ref U6) (pin 64)))
    (net (code 47) (name "Net-(U6-Pad65)")
      (node (ref U6) (pin 65)))
    (net (code 48) (name "Net-(U6-Pad66)")
      (node (ref U6) (pin 66)))
    (net (code 49) (name "Net-(J11-Pad3)")
      (node (ref U6) (pin 42))
      (node (ref J11) (pin 3)))
    (net (code 50) (name "Net-(J10-Pad3)")
      (node (ref U6) (pin 43))
      (node (ref J10) (pin 3)))
    (net (code 51) (name "Net-(U6-Pad67)")
      (node (ref U6) (pin 67)))
    (net (code 52) (name "Net-(J9-Pad3)")
      (node (ref J9) (pin 3))
      (node (ref U6) (pin 44)))
    (net (code 53) (name "Net-(J8-Pad3)")
      (node (ref J8) (pin 3))
      (node (ref U6) (pin 45)))
    (net (code 54) (name "Net-(J7-Pad3)")
      (node (ref J7) (pin 3))
      (node (ref U6) (pin 46)))
    (net (code 55) (name "Net-(U1-Pad8)")
      (node (ref U1) (pin 8))
      (node (ref U6) (pin 15)))
    (net (code 56) (name "Net-(U6-Pad29)")
      (node (ref U6) (pin 29)))
    (net (code 57) (name "Net-(U6-Pad79)")
      (node (ref U6) (pin 79)))
    (net (code 58) (name "Net-(U6-Pad68)")
      (node (ref U6) (pin 68)))
    (net (code 59) (name "Net-(U6-Pad69)")
      (node (ref U6) (pin 69)))
    (net (code 60) (name "Net-(U6-Pad70)")
      (node (ref U6) (pin 70)))
    (net (code 61) (name "Net-(U6-Pad71)")
      (node (ref U6) (pin 71)))
    (net (code 62) (name "Net-(U6-Pad72)")
      (node (ref U6) (pin 72)))
    (net (code 63) (name "Net-(U6-Pad73)")
      (node (ref U6) (pin 73)))
    (net (code 64) (name "Net-(U6-Pad74)")
      (node (ref U6) (pin 74)))
    (net (code 65) (name "Net-(U6-Pad75)")
      (node (ref U6) (pin 75)))
    (net (code 66) (name "Net-(U6-Pad76)")
      (node (ref U6) (pin 76)))
    (net (code 67) (name "Net-(U6-Pad77)")
      (node (ref U6) (pin 77)))
    (net (code 68) (name "Net-(U6-Pad78)")
      (node (ref U6) (pin 78)))
    (net (code 69) (name "Net-(U6-Pad80)")
      (node (ref U6) (pin 80)))
    (net (code 70) (name "Net-(U6-Pad81)")
      (node (ref U6) (pin 81)))
    (net (code 71) (name "Net-(U6-Pad82)")
      (node (ref U6) (pin 82)))
    (net (code 72) (name "Net-(U6-Pad83)")
      (node (ref U6) (pin 83)))
    (net (code 73) (name "Net-(U6-Pad84)")
      (node (ref U6) (pin 84)))
    (net (code 74) (name "Net-(U6-Pad85)")
      (node (ref U6) (pin 85)))
    (net (code 75) (name "Net-(U6-Pad25)")
      (node (ref U6) (pin 25)))
    (net (code 76) (name "Net-(U6-Pad26)")
      (node (ref U6) (pin 26)))
    (net (code 77) (name "Net-(U6-Pad27)")
      (node (ref U6) (pin 27)))
    (net (code 78) (name "Net-(U6-Pad28)")
      (node (ref U6) (pin 28)))
    (net (code 79) (name "Net-(J15-Pad3)")
      (node (ref U6) (pin 34))
      (node (ref J15) (pin 3)))
    (net (code 80) (name "Net-(J14-Pad3)")
      (node (ref J14) (pin 3))
      (node (ref U6) (pin 35)))
    (net (code 81) (name "Net-(J13-Pad3)")
      (node (ref U6) (pin 36))
      (node (ref J13) (pin 3)))
    (net (code 82) (name "Net-(J12-Pad3)")
      (node (ref U6) (pin 41))
      (node (ref J12) (pin 3)))
    (net (code 83) (name "Net-(J19-Pad3)")
      (node (ref J19) (pin 3))
      (node (ref U6) (pin 30)))
    (net (code 84) (name "Net-(J18-Pad3)")
      (node (ref U6) (pin 31))
      (node (ref J18) (pin 3)))
    (net (code 85) (name "Net-(J17-Pad3)")
      (node (ref J17) (pin 3))
      (node (ref U6) (pin 32)))
    (net (code 86) (name "Net-(J16-Pad3)")
      (node (ref J16) (pin 3))
      (node (ref U6) (pin 33)))
    (net (code 87) (name "Net-(U1-Pad2)")
      (node (ref U1) (pin 2))
      (node (ref U6) (pin 13)))
    (net (code 88) (name "Net-(U6-Pad58)")
      (node (ref U6) (pin 58)))
    (net (code 89) (name "Net-(U1-Pad6)")
      (node (ref U6) (pin 14))
      (node (ref U1) (pin 6)))
    (net (code 90) (name "Net-(U1-Pad3)")
      (node (ref U1) (pin 3))
      (node (ref U6) (pin 19)))
    (net (code 91) (name "Net-(U1-Pad5)")
      (node (ref U1) (pin 5)))
    (net (code 92) (name "Net-(U1-Pad7)")
      (node (ref U1) (pin 7)))
    (net (code 93) (name "Net-(U2-Pad13)")
      (node (ref U2) (pin 13)))
    (net (code 94) (name "Net-(U2-Pad11)")
      (node (ref U2) (pin 11)))
    (net (code 95) (name "Net-(J2-Pad1)")
      (node (ref U2) (pin 3))
      (node (ref J2) (pin 1)))
    (net (code 96) (name "Net-(J2-Pad3)")
      (node (ref J2) (pin 3))
      (node (ref U2) (pin 6)))
    (net (code 97) (name "Net-(J2-Pad5)")
      (node (ref U2) (pin 8))
      (node (ref J2) (pin 5)))
    (net (code 98) (name "Net-(U6-Pad86)")
      (node (ref U6) (pin 86)))
    (net (code 99) (name "Net-(J4-Pad5)")
      (node (ref J4) (pin 5))
      (node (ref U4) (pin 8)))
    (net (code 100) (name "Net-(J4-Pad3)")
      (node (ref U4) (pin 6))
      (node (ref J4) (pin 3)))
    (net (code 101) (name "Net-(J4-Pad1)")
      (node (ref U4) (pin 3))
      (node (ref J4) (pin 1)))
    (net (code 102) (name "Net-(U4-Pad13)")
      (node (ref U4) (pin 13)))
    (net (code 103) (name "Net-(U4-Pad11)")
      (node (ref U4) (pin 11)))
    (net (code 104) (name "Net-(U5-Pad13)")
      (node (ref U5) (pin 13)))
    (net (code 105) (name "Net-(U5-Pad11)")
      (node (ref U5) (pin 11)))
    (net (code 106) (name "Net-(U3-Pad13)")
      (node (ref U3) (pin 13)))
    (net (code 107) (name "Net-(U3-Pad11)")
      (node (ref U3) (pin 11)))
    (net (code 108) (name "Net-(J3-Pad1)")
      (node (ref J3) (pin 1))
      (node (ref U3) (pin 3)))
    (net (code 109) (name "Net-(J3-Pad3)")
      (node (ref U3) (pin 6))
      (node (ref J3) (pin 3)))
    (net (code 110) (name "Net-(J3-Pad5)")
      (node (ref U3) (pin 8))
      (node (ref J3) (pin 5)))))