#N canvas 1 53 450 377 10;
#X obj 52 180 dac~;
#X obj 53 143 *~;
#X obj 53 79 tgl 15 0 empty empty empty 17 7 0 10 -4034 -13381 -1 0
1;
#X obj 80 79 nbx 5 14 0 1e+37 0 1 empty empty seconds 60 8 0 10 -4034
-13381 -13381 0.73 256;
#X obj 53 57 metro 1000;
#X obj 53 36 tgl 15 0 empty empty empty 17 7 0 10 -4034 -13381 -1 0
1;
#X obj 53 99 rc~ 1;
#X text 191 167 Author: Martin Peach;
#X text 191 186 2010/03/15;
#X obj 67 121 noise~;
#X obj 136 230 lop~;
#X text 63 230 similar to:;
#X text 49 -22 rc~ emulates a capacitor charging through a resistor.
The creation argument can be overriden by the right inlet \, and represents
a charging time constant in seconds.;
#N canvas 453 86 494 344 META 0;
#X text 12 145 HELP_PATCH_AUTHORS "pd meta" information added by Jonathan
Wilkes for Pd version 0.42.;
#X text 12 25 LICENSE GPL v2 or later;
#X text 12 125 AUTHOR Martin Peach;
#X text 12 46 DESCRIPTION emulate a capacitor charging through a resistor
;
#X text 12 65 INLET_0 float;
#X text 12 85 INLET_1 float;
#X text 12 105 OUTLET_0 signal;
#X text 12 5 KEYWORDS signal;
#X restore 379 329 pd META;
#X connect 1 0 0 0;
#X connect 1 0 0 1;
#X connect 2 0 6 0;
#X connect 3 0 6 1;
#X connect 4 0 2 0;
#X connect 5 0 4 0;
#X connect 6 0 1 0;
#X connect 9 0 1 1;
