#N canvas 665 293 742 610 12;
#X floatatom 414 304 3 0 0 0 - - -, f 3;
#X floatatom 441 304 3 0 0 0 - - -, f 3;
#X floatatom 468 304 3 0 0 0 - - -, f 3;
#X floatatom 495 304 3 0 0 0 - - -, f 3;
#X floatatom 522 305 5 0 0 0 - - -, f 5;
#X obj 414 278 unpack 0 0 0 0 0;
#X msg 191 90 status;
#X floatatom 293 225 9 0 0 0 - - -, f 9;
#X obj 474 251 tgl 15 0 empty empty empty 17 7 0 10 -4034 -1 -1 0 1
;
#X floatatom 353 251 9 0 0 0 - - -, f 9;
#X text -10 90 get status on right outlet:;
#X text 186 225 bytes received:;
#X text 201 249 total bytes received:;
#X text 371 303 from:;
#X text 293 78 Specify a multicast address (from 224.0.0.0 to 239.255.255.255)
to use multicasting;
#X text 36 38 Creation arguments: port number to listen on (required)
;
#X obj 230 274 tgl 15 0 empty empty enable_print: -77 8 0 10 -4034
-1 -1 0 1;
#X obj 234 344 print received;
#X obj 293 192 route received total from multicast;
#X text 175 56 IP address to listen on (optional);
#X msg 202 129 port 9998;
#X text 276 127 change port to listen on;
#X text 486 360 Martin Peach 2010/10/15;
#X text -12 3 [udpreceive] receives datagrams over a udp connection
and outputs them as raw bytes.;
#N canvas 529 53 494 344 META 0;
#X text 12 155 HELP_PATCH_AUTHORS "pd meta" information added by Jonathan
Wilkes for Pd version 0.42.;
#X text 12 25 LICENSE GPL v2 or later;
#X text 12 135 AUTHOR Martin Peach;
#X text 12 5 KEYWORDS control network;
#X text 12 45 DESCRIPTION receive datagrams over a udp connection and
outputs them as raw bytes;
#X text 12 75 INLET_0 status port;
#X text 12 95 OUTLET_0 anything;
#X text 12 115 OUTLET_1 received total from multicast;
#X restore 657 396 pd META;
#X obj 191 294 unpackOSC;
#X obj 191 160 udpreceive 9000;
#X obj 78 236 udpsend 8000;
#X obj 81 202 spigot;
#X obj 136 166 tgl 15 0 empty empty empty 17 7 0 10 -262144 -1 -1 0
1;
#X msg 47 352 connect 127.0.0.1 8000;
#X obj 114 319 packOSC;
#X obj 215 400 vsl 15 128 0 1024 0 0 empty empty empty 0 -9 0 10 -1
-4034 -1 12588 1;
#X obj 191 319 route /analog/0;
#X connect 5 0 0 0;
#X connect 5 1 1 0;
#X connect 5 2 2 0;
#X connect 5 3 3 0;
#X connect 5 4 4 0;
#X connect 6 0 26 0;
#X connect 18 0 7 0;
#X connect 18 1 9 0;
#X connect 18 2 5 0;
#X connect 18 3 8 0;
#X connect 20 0 26 0;
#X connect 25 0 17 0;
#X connect 25 0 31 0;
#X connect 25 0 33 0;
#X connect 26 0 25 0;
#X connect 26 1 18 0;
#X connect 28 0 27 0;
#X connect 29 0 28 1;
#X connect 30 0 27 0;
#X connect 31 0 28 0;
#X connect 33 0 32 0;
